Read head

 Micron-P2 - CR - 20 - SX - 0.5

Cable length:

0.5: 0.5 meters

Customized length

Disk material and code:

S: stainless steel; G: glass(n/a for now)

X: disk code

Interpolation factor:

20:20X

refer to disk selection manual

Package type & scale type

C: closed/sealed housing; B: bare PCB

R: rotary

Series No.

P2: 20µm grating pitch

Scale

GS20 - R - S52

Series No.

20: 20µm grating

Scale type:

R: Rotary

Disk material

S: stainless steel

G: glass (n/a for now)

Disk code:

52: disk outer diameter(DO=52.2/52.1 mm)

200: disk outer diameter(DO=200.4/200.2 mm)